**4.9 STEERING WHEELS**

Replacement steering wheels must not affect compliance with ADR 10 (after 1970) and ADR 69

(after June 1995). Unless a steering wheel is marked, or has accompanying information, as

having been tested to the appropriate ADR, it must not be used as a replacement. In addition,

for vehicles required to comply with ADR 69, the steering wheel assembly must be identical to

one fitted as an option to the same model by the vehicle manufacturer, or alternatively, a

steering wheel that has been certified by the replacement wheel manufacturer as a complying

wheel for the specific make and model may be used.

Replacement steering wheels should not be less than 330mm in diameter. If the original

steering wheel was designed with a recessed or padded hub, the replacement wheel should be

of a similar design.

Removable steering wheels must not be fitted